/*
    FreeRTOS V6.0.4 - Copyright (C) 2010 Real Time Engineers Ltd.

    ***************************************************************************
    *                                                                         *
    * If you are:                                                             *
    *                                                                         *
    *    + New to FreeRTOS,                                                   *
    *    + Wanting to learn FreeRTOS or multitasking in general quickly       *
    *    + Looking for basic training,                                        *
    *    + Wanting to improve your FreeRTOS skills and productivity           *
    *                                                                         *
    * then take a look at the FreeRTOS eBook                                  *
    *                                                                         *
    *        "Using the FreeRTOS Real Time Kernel - a Practical Guide"        *
    *                  http://www.FreeRTOS.org/Documentation                  *
    *                                                                         *
    * A pdf reference manual is also available.  Both are usually delivered   *
    * to your inbox within 20 minutes to two hours when purchased between 8am *
    * and 8pm GMT (although please allow up to 24 hours in case of            *
    * exceptional circumstances).  Thank you for your support!                *
    *                                                                         *
    ***************************************************************************

    This file is part of the FreeRTOS distribution.

    FreeRTOS is free software; you can redistribute it and/or modify it under
    the terms of the GNU General Public License (version 2) as published by the
    Free Software Foundation AND MODIFIED BY the FreeRTOS exception.
    ***NOTE*** The exception to the GPL is included to allow you to distribute
    a combined work that includes FreeRTOS without being obliged to provide the
    source code for proprietary components outside of the FreeRTOS kernel.
    FreeRTOS is distributed in the hope that it will be useful, but WITHOUT
    ANY WARRANTY; without even the implied warranty of MERCHANTABILITY or
    FITNESS FOR A PARTICULAR PURPOSE.  See the GNU General Public License for
    more details. You should have received a copy of the GNU General Public 
    License and the FreeRTOS license exception along with FreeRTOS; if not it 
    can be viewed here: http://www.freertos.org/a00114.html and also obtained 
    by writing to Richard Barry, contact details for whom are available on the
    FreeRTOS WEB site.

    1 tab == 4 spaces!

    http://www.FreeRTOS.org - Documentation, latest information, license and
    contact details.

    http://www.SafeRTOS.com - A version that is certified for use in safety
    critical systems.

    http://www.OpenRTOS.com - Commercial support, development, porting,
    licensing and training services.
*/

#ifndef FREERTOS_CONFIG_H
#define FREERTOS_CONFIG_H

#include "MCF52235.h"

/*-----------------------------------------------------------
 * Application specific definitions.
 *
 * These definitions should be adjusted for your particular hardware and
 * application requirements.
 *
 * THESE PARAMETERS ARE DESCRIBED WITHIN THE 'CONFIGURATION' SECTION OF THE
 * FreeRTOS API DOCUMENTATION AVAILABLE ON THE FreeRTOS.org WEB SITE.
 *
 * See http://www.freertos.org/a00110.html.
 *----------------------------------------------------------*/

#define configUSE_PREEMPTION			1
#define configUSE_IDLE_HOOK				1
#define configUSE_TICK_HOOK				0
#define configCPU_CLOCK_HZ				( ( unsigned long ) 60000000 )
#define configTICK_RATE_HZ				( ( portTickType ) 1000 )
#define configMINIMAL_STACK_SIZE		( ( unsigned short ) 100 )
#define configTOTAL_HEAP_SIZE			( ( size_t ) ( 19000 ) )
#define configMAX_TASK_NAME_LEN			( 12 )
#define configUSE_TRACE_FACILITY		1
#define configUSE_16_BIT_TICKS			0
#define configIDLE_SHOULD_YIELD			0
#define configUSE_CO_ROUTINES 			0
#define configUSE_MUTEXES				1
#define configCHECK_FOR_STACK_OVERFLOW	2 //1 prestav
#define configUSE_RECURSIVE_MUTEXES		1
#define configQUEUE_REGISTRY_SIZE		10
#define configUSE_COUNTING_SEMAPHORES	1

#define configMAX_PRIORITIES		( ( unsigned portBASE_TYPE ) 6 )
#define configMAX_CO_ROUTINE_PRIORITIES ( 2 )

/* Set the following definitions to 1 to include the API function, or zero
to exclude the API function. */

#define INCLUDE_vTaskPrioritySet			1
#define INCLUDE_uxTaskPriorityGet			1
#define INCLUDE_vTaskDelete					1
#define INCLUDE_vTaskCleanUpResources		0
#define INCLUDE_vTaskSuspend				1
#define INCLUDE_vTaskDelayUntil				1
#define INCLUDE_vTaskDelay					1
#define INCLUDE_uxTaskGetStackHighWaterMark	1

/* Port specific definitions. */
#define configYIELD_INTERRUPT_VECTOR			16UL
#define configKERNEL_INTERRUPT_PRIORITY 		1
#define configMAX_SYSCALL_INTERRUPT_PRIORITY 	4

/* The function that initialises the tick and context switch interrupts.  This
function is part of the application side (rather than kernel) to allow users to
change the peripherals and vectors being used should they conflict in any way
with the application itself. */
void vApplicationSetupInterrupts( void );

/* Ethernet configuration. **************************/

/* Defines the MAC address to be used. */
#define configMAC_0	0x00
#define configMAC_1	0x04
#define configMAC_2	0x9F
#define configMAC_3	0x00
#define configMAC_4	0xAB
#define configMAC_5	0x2B

/* Defines the IP address to be used. */
#define configIP_ADDR0	10
#define configIP_ADDR1	0
#define configIP_ADDR2	0
#define configIP_ADDR3	150

/* Defines the gateway address to be used. */
#define configGW_ADDR0	10
#define configGW_ADDR1	0
#define configGW_ADDR2	0
#define configGW_ADDR3	1

/* Defins the net mask. */
#define configNET_MASK0	255
#define configNET_MASK1	255
#define configNET_MASK2	255
#define configNET_MASK3	0

/* FEC driver configuration. */
#define configNUM_FEC_RX_BUFFERS	3
#define configFEC_BUFFER_SIZE		1520
#define configUSE_PROMISCUOUS_MODE	0
#define configFEC_INTERRUPT_PRIORITY configMAX_SYSCALL_INTERRUPT_PRIORITY
#define configPHY_ADDRESS	0

#if ( configFEC_BUFFER_SIZE & 0x0F ) != 0
	#error configFEC_BUFFER_SIZE must be a multiple of 16.
#endif


#endif /* FREERTOS_CONFIG_H */
